Setup ADC

Write factors to FLASH

Read calibration factors from (1 and 2) from the memory

Measure and store measured ADC1 and ADC2 values

Start/Reset

Set SPI and/or UART connection

Display both ADC values

Configurate potentiometers’ pins